To anchor pole:

* Place threaded rod tip on ice 10” back from hole.
* With one hand, grasp the vertical main body about 2/3 of the way up and apply pressure straight down.

With the other hand, grasp the black cap on top of the U-Bend and rotate the pole clockwise until the IceGrip stands on its own. This should take approximately 12 turns or until the pole is anchored to the desired tightness or the nut touches the ice. Do NOT apply downward pressure with the cranking hand.

To remove pole:

* Grasp the black cap on top of the U-Bend and rotate the pole counter-clockwise until anchor tip is out of the ice.

Configurations:

* The rig can accommodate up to two combo set-ups for jigging simultaneously with two mounted reels for hand-landing or up to four mounted reels of your choice.

To mount reel (advisable to do before anchoring pole):

* Slide keeper O-rings out of the way and slide rubber grommets to a width wider than your selected reel base.
* Hold reel base tight to the bottom of tube and use slight twist motion to push back grommet onto reel until it is flush with the reel shoulder. Repeat for front grommet.
* O-Rings are not needed to mount the reel. They only act as a keeper for grommets when no reel is on the tube. Push them back tight to reel if desired.

To use jigging poles:

* Slide O-rings (and grommets if applicable) to a width wider than your selected jigging pole.
* Set jigging pole on rig to locate balance point.
* OPTIONAL: Fasten clip (zip-tie) to handle in front of balance point. The clip is an added safety measure to ensure that your rod will stay in place, but is not required.

Lubricate Grommets:

* For the initial few uses, apply a small amount of oil or water on the tube and then rotate the grommets. Wipe off all remaining excess oil/water from tube. This will allow grommets to slide on the reel base more easily when mounting reels.

Flagging:

* After anchoring the pole on the ice, drop your line through the U-bend and into the hole to the desired depth, then cut off 10-40” of flagging and tie a knot to the line (or end of jigging pole if desired).

OTHER PRO TIPS & FAQs:

* Can I use the IceGrip in other materials? *Yes! While it was built for ice, it also works in wood and shorelines.*
* Should I be worried about pancaking? *No!* Even on super hard subzero ice, IceGrip's auger bolt will install easily and avoid "pancaking"
* What if I’m ice fishing in warmer temperatures? *IceGrip can be used in all temperatures, including those above-freezing sunny days.*
* Can I leave the IceGrip in overnight? *Yes. IceGrip can still be easily removed even after being left anchored overnight or out in a deep freeze.*
* Can I use this with my existing equipment? *Yes. IceGrip is intended to be compatible with all rods, reels and combo setups on the market today.*
* Tell me more about flagging. *You can slide the flag up and down line to set depth as desired.* *When the flag disappears under ice, you are ready to go make a set!*